**EarthCam ConstructionCam HD Model # ECCS01127 A&E Specifications**

**01.32.36 Video Monitoring and Documentation**

1. **CAMERA SPECIFICATIONS**
   1. **Contractor Contact Information**

The Contractor shall provide a Robotic High Definition Megapixel Webcam for users to remotely view the project on a secure connection via a network connection. The camera will provide a full view of the work area on the construction site.

CONTACT SYSTEM VENDOR: EarthCam Inc. / Brian Cury +1 201.488.1111

Email: WWW.EARTHCAM.NET/CONTACTUS

* 1. **Camera System for Highest Precision Monitoring and Documentation**
     + 1. Consist of a thermostatically controlled environmentally sealed enclosure
       2. Camera Enclosure Dimensions: 26.695” (678mm) H x 8.661” (220mm) W x 20.75” (527mm) D
       3. Weight: Camera: 13lb (5.9kg), Pan/Tilt Unit: 9lb (4.1kg)
       4. User controlled window wiper
       5. Industrial grade solid state embedded Linux System
       6. Precise, Pan/Tilt robotic base designed to provide consistent imaging in all environments
       7. Pan/Tilt Unit Dimensions: 11.3” (288mm) H x 6.5” (165mm) W x 7.4” (189mm) D
       8. Capable of maintaining multiple preset compositions
       9. Live video stream in H.264 format
       10. 1080p broadcast quality video clip capability
       11. H.264, MPEG-4 Part 10/AVC, Motion JPEG video compression
       12. 50/60fps in all resolutions
       13. 2.1 Megapixel images (1920 x 1080 pixels)
       14. Up to 150 Megapixels auto-generated 360° panoramas
       15. Lens: 3.8 – 38mm, f/1.8 – 3.4, 10X Optical, 12X Digital, HD image sensor
       16. 67.8° angle of view
       17. Auto Features: Focus and Day/Night
       18. Communications: RJ-45 10BASE-T/100BASE-TX PoE
       19. 4G cellular modem
       20. 16GB On-Board Data Back-Up to provide a minimum of thirty days of on-board image retention
       21. 120VAC, 220-230VAC or 12VDC power
       22. Designed for EarthCam Control Center Software

1. **SERVICE SPECIFICATIONS**
   1. **Internet Based Online Interface**

The camera will be accessible via an internet based Software as a Service (SaaS) solution. This online interface will be managed and supported by the System Vendor. The service will be available for the term of the project and allow the viewing of live video and High Definition digital still images captured and stored of the project on both mobile and desktop platforms.

The Internet Based Online Interface shall include the following features:

* + 1. Responsive HTML5 design for cross-platform access on desktop and mobile devices
    2. Display project name and logo
    3. Project Dashboard for viewing and accessing multiple cameras
    4. Real-time live video viewing
    5. User-controllable Robotic Pan, Tilt and Zoom
    6. User-controllable settings for creating and editing multiple preset compositions
    7. Automatically generated daily panoramas
    8. Monthly and on demand ultra HD panoramas
    9. Onscreen control button for wiper control to allow for remote cleaning of the viewing window
    10. Picture in picture capability for viewing live video and High Definition Megapixel images simultaneously
    11. Digital Pan, Tilt and Zoom capability within a High Definition image
    12. Instant live snapshot capability in addition to preset scheduled archives
    13. Timeline navigation system for selecting specific images and times
    14. Multifunction Image Browsing
    15. Time-lapse feature with optional time date overlay for instant time-lapse viewing, downloading and embedding
    16. Full Screen Mode for displaying video and complete image without any graphical frame
    17. Photo Filters and Graphical Markup Tools for detailing and creating notes with graphical overlays on images, including project title, logo and time date stamp
    18. Image Comparison Tool for comparing two images taken at different times, overlayed on top of each other
    19. Share Image Tool for saving, printing, emailing and posting to Hall of Fame
    20. Marketing Section for posting and sharing camera images with notes
    21. Social Media Integration Tools for sharing project images and notes on Facebook and Twitter
    22. Automatically generated daily/weekly project progress update email with camera image and weather
    23. Graphical Weather applet displaying local weather data with satellite and updating radar imaging
    24. Integration of maps, aerial and satellite imagery
    25. Graphical Data Management Tools showing archived and current system status of solar amperage, battery power remaining, wireless radio connectivity, and device location
  1. **Security and Management**
     1. Access to account protected by Account Security feature which includes four levels of password protection, IP address block/permission and SSL protection of user login password.
     2. The system shall capture and upload images every 5 minutes, 24 hours per day.
     3. The system shall have M2M – Machine to Machine 24/7 Support with active self-healing technology and automatic software upgrades to maintain the quality, consistency and reliability of all images.
     4. Images will be maintained on the System Vendor’s servers for reference available at all times during the life of the project and for no less than 60 days after completion. All images will be protected on servers owned and operated by the System Vendor and located in a secure area at the System Vendor’s location.

1. **CONTRACTOR REQUIREMENTS** 
   1. **Jobsite Requirements**

The Contractor shall secure a nearby structure for camera mounting or provide a fixed pole (40 foot / 12 meters height recommended) and 3 inch / 8 centimeters minimum diameter as per System Vendor’s instruction. The Contractor shall supply all equipment required for safe and secure access to the camera location for technicians performing installation and maintenance services, including building access, bucket truck and/or lift. The System Vendor will consult on and provide recommendations for optimal camera placement and provide professional installation services as required.

* 1. **Camera Maintenance**

The Contractor shall provide all service and maintenance, including cleaning, of the camera system throughout the life of the project including making appropriate arrangements for camera to remain in operation up to and through finalization of all structural, landscaping and “completed state” condition necessary for beginning-to-end time-lapse record.

1. **DELIVERABLES** 
   1. **Public Website**

The System Vendor shall provide custom public website development. Website shall be separate from the Online Interface, match the look and colors of the project’s website, and be delivered as embed code or standalone web page. Additional features include Facebook and Twitter integration, full screen mode, image comparison, weather, multiple logos, graphical background image and project description.

* 1. **End of Project Time-Lapse Movie**

The System Vendor shall provide time-lapse movie(s) at the end of the project. Time-lapses shall be professionally edited by a video editor using image stabilization software. The movie will start with a graphic, incorporating project title, date and logo. Periods of bad weather or inactivity shall be removed to produce a compelling and consistent movie. A machine edited movie will not be acceptable.